[image: image1.png]


KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
[image: image7.png]WWWWWWWWWWWWWW



  TEL/WhatsApp: +86 17622605414
Mail: admin@transformercoilwindingmachine.com
    Web:www.transformercoilwindingmachine.com

NAME:ACKX22-1A Voice coil winding machine
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Specifications

	Spindle number
	1

	Wire size range
	0.05-1.7mm

	Loop diameter
	200mm

	Max wire distance
	9.99mm

	Winder width
	180mm

	Max speed
	0-4000 RPM

	Spindle motor
	Three Phase motor+AC Drives

	Winder motor
	Stepping motor

	Input power
	220V  50HZ/60HZ

	Machine size
	600×360×450mm

	Package size
	750×470×620mm

	Net weight
	60kg

	Gross weight
	83kg


Features： 

Voice coil winding machine uses the latest synchronization with the coupling cable controller. 

voice coil winding processing with self detection, including setting error, speed tracking and velocity calibration.
Optional lifting speed of main spindle.
Start moving speed of the spindle motor to climb time to decide. 

The tension of the special design for speaker coil winding machine , greatly enhance the winding effect.. 
Advantages:

Professional winding big wire size products, large torque, good winding effect. 

Voice coil winding machine designed of 32 bit controller chip, It’ll be faster and higher reliability.

In Chinese and English display,easy to operation,winding data retention after power failure, not to discarded products.
All the parts for this machine are imported prats,such as:Japan Bearing (NSK、NTN),Japan BANDO belt ，U.S.A GATES belt ，Taiwan Ball screw (TBI)，Taiwan AC Drive and so on.
APPLICATION:

The ACKX22-1A Voice Coil Winding Machine is specifically designed for manufacturing high-precision voice coils, making it ideal for manufacturing components critical to audio equipment such as speakers and headphones. Unlike toroid winding machines, which are best suited for toroidal inductors, toroidal transformers, toroidal current transformers, toroidal coils, toroid choke coils, power inductors, UPS inductors, converter inductors, and heavy toroidal cores, the ACKX22-1A focuses on the precise, delicate winding required for voice coils.

Its specialized design caters to the unique needs of voice coil production, including handling fine wires, maintaining uniform winding density, and ensuring consistent layer alignment—all essential for optimal acoustic performance in audio devices. This focus on audio component manufacturing distinguishes it from toroid winding equipment, which is tailored for industrial electrical components.
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PRACTICAL APPLICATION :

Training for Customers to Operate ACKX22-1A Voice Coil Winding Machine

1.All service engineers with 10 years of experience have received special technical training, including specialized expertise in the ACKX22-1A Voice Coil Winding Machine, enabling them to effectively handle various breakdown issues specific to this precision audio component equipment, such as fine wire tension control failures for fine wires, alignment errors in voice coil layers, or programming glitches in the winding sequence.

2.We guide users to accurately operate and maintain the ACKX22-1A Voice Coil Winding Machine—with focused attention to its fine wire threading procedures, voice coil parameter setting (including turns count and wire spacing), calibration of winding precision, and maintenance of delicate components like wire guides and tensioners—while providing free consultation about the production process technology related to electronic voice coil manufacturing, including optimal techniques for different wire gauges and voice coil specifications.

3.To ensure the ACKX22-1A Voice Coil Winding Machine operates normally, we conduct dedicated training on its specialized functions, step-by-step operational procedures for voice coil production, and preventive maintenance protocols through English manuals, model-specific instructional videos, and real-time online guidance—all tailored to the unique requirements of this precision voice coil winding equipment.
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PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for Voice coil winding machine      

, Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale Eight Spindle Voice coil winding machine  ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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FACTORY:

We, KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD. have been experts in winding machine lines for 28 years, with our specialized product portfolio including precision equipment like the ACKX22-1A Voice Coil Winding Machine—a state-of-the-art system engineered for manufacturing high-quality voice coils, showcasing our technical prowess in specialized audio component winding solutions.

Our KIOXIA LIGHT RING brand holds authoritative certifications and recognitions, including ISO9001:2015, CE approvals, multiple machine patents (encompassing key innovations in models like the ACKX22-1A Voice Coil Winding Machine), and the official designation of "high-tech enterprise" by the government. These credentials validate the reliability, precision, and technical excellence of our entire product range, reinforcing our commitment to delivering advanced winding solutions for diverse applications, including the specialized field of voice coil production.
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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

